EEE Project v 1.7.0
-------------------

EEE Project was developed with NI LabVIEW 8.2.1, and LV Run-Time Engine v8.2.1 must be
installed before any other EEE application.

Please install CAEN VME Demo as it will install CAENVMElib.dll required for EEE Data Acquisition
and EEE HW Address Checker programs.

IMPORTANT: This version requires CAEN TDC V1190 firmware Rev0.7 or later. Please update firmware on each TDC in the system!
EEE Pulse Width Converter uses new functionality provided by this update, and therefore cannot be used to process old data files.

New in version 1.7.0
--------------------

1. EEE Data Acquisition:
- Geometry page added, please check and modify parameters for your station;
- Geometry, Match Window and Delay information stored in binary file, please refer to EEE BIN Format v1.7.0.xls;
- automatic Convert to TXT at the end of acquisition removed, please use EEE TXT Converter instead;
- Fast Restart added to skip TDC re-configuration in Auto Restart mode;

2. EEE Histogram Builder:
- Parameters page added;
- Comment and Mode And Resolution indicators moved to Parameters page;
- Geometry, Match Window and Delay information is shown on Parameters page if present in binary file;

3. EEE TXT Converter:
- output TXT file shows Geometry, Match Window and Delay information if present in binary file;

4. EEE Pulse Width Converter:
- in Time conversion mode takes into account delay between 1PPS trigger and CLR signal to calculate calibration coefficients


In case of software installation problem please contact Raman Zuyeuski at CERN:

E-mail: Raman.Zuyeuski@cern.ch
Phone: +41 (22) 767 7596
